|  |  |
| --- | --- |
|  | **Half or Full-Face Respirator**  **Protects- You, NOT others.**  **Required Use: Installation of 2-part spray foam and Lead Safe Practices. Areas of a home that may have organic vapors present.**  **Recommended use: P100 cartridge for demolition and installing insulation.**  **Worn By: Installers and sometimes Auditors/QCI** |
|  | **N95 Face Mask**  **Protects- You and others around you**  **Required Use: Minimum protection from airborne contaminants (e.g., insulation materials, mold spores, feces, bacteria, chemicals.**  **Filters 95% of airborne particles.**  **Worn During: Coach visit, Auditing/QCI, Installation of Materials, when a dusty environment is present during inspections or working in (e.g., attics, crawlspace, basements, and under mobile homes.** |
|  | **Cloth Face Mask**  **Protects- Others, but NOT necessarily you**  **Required Use: At the office/shop, in work vehicles, public places, at work site.**  **These masks shall be worn for protecting against the spread of viruses and diseases during working hours.**  **Worn By: All Staff members**  **Example: client/co-worker interaction, tasks that do not create dust, but others are present.** |
|  | **Respirator Cartridges**  **Protects-You NOT others**  **Cartridges shall be NIOSH approved**  **Type: OV/P100 is a combination cartridge that protects the user from organic vapor and 99.97% of airborne particles. P100 protects the user from 99.97% of airborne particles.**  **OV/P100 Required when installing 2-part spray foam.**  **P100 Only Recommended in dusty environments.** |