|  |  |
| --- | --- |
|  | **Half or Full-Face Respirator****Protects- You, NOT others.****Required Use: Installation of 2-part spray foam and Lead Safe Practices. Areas of a home that may have organic vapors present.****Recommended use: P100 cartridge for demolition and installing insulation.****Worn By: Installers and sometimes Auditors/QCI** |
|  | **N95 Face Mask****Protects- You and others around you****Required Use: Minimum protection from airborne contaminants (e.g., insulation materials, mold spores, feces, bacteria, chemicals.** **Filters 95% of airborne particles.****Worn During: Coach visit, Auditing/QCI, Installation of Materials, when a dusty environment is present during inspections or working in (e.g., attics, crawlspace, basements, and under mobile homes.**  |
|  | **Cloth Face Mask****Protects- Others, but NOT necessarily you****Required Use: At the office/shop, in work vehicles, public places, at work site.****These masks shall be worn for protecting against the spread of viruses and diseases during working hours.****Worn By: All Staff members****Example: client/co-worker interaction, tasks that do not create dust, but others are present.** |
|  | **Respirator Cartridges****Protects-You NOT others****Cartridges shall be NIOSH approved****Type: OV/P100 is a combination cartridge that protects the user from organic vapor and 99.97% of airborne particles. P100 protects the user from 99.97% of airborne particles.****OV/P100 Required when installing 2-part spray foam.****P100 Only Recommended in dusty environments.** |