**Auditor Tool and Equipment List**

**Diagnostic Equipment:**

* Blower Door kit
* IR imager
* Manometers and hoses
* Combustion Analyzer (measures CO, oxygen and temperature)
* Hand held CO detector (if not a feature on combustion analyzer)
* Gas leak detector
* Smoke generating device
* Probe thermometers
* Pressure pan
* Exhaust fan flow meter
* “Watts Up” meter
* Inspection mirrors.
* Bore scope
* Digital camera (most will bring their own)
* Pads of paper and pencils

**Assorted Tools and Material:**

* + Telescoping ladder – lightweight and convenient; easy to maneuver in tight quarters.
	+ Cordless drill with drill bits and assorted drivers
	+ Long probe gas grill lighter
	+ Non contact voltage detector
	+ Phillips head and slotted screwdrivers.
	+ Cutting pliers.
	+ Regular gripping pliers
	+ Hammer
	+ Awl punch
	+ Adjustable wrench.
	+ Assorted fasteners
	+ Box Cutter.
	+ 25’ tape measure.
	+ Flashlight
	+ Utility light (electric)
	+ Plastic crochet hook (for fishing insulation samples through small openings).
	+ Clear sticky duct masking (to cover registers)
	+ Wide painters masking tape
	+ Duct tape
	+ Electrical tape
	+ Extension cord in 25 or 50 foot lengths
	+ Power strip
	+ Three prong electrical outlet adapter

PPE:

* Tyvec suits
* Roll plastic
* Hand sanitizer
* Protective eye glasses
* Industrial first aid kit
* Line voltage detector