**Auditor Tool and Equipment List**

**Diagnostic Equipment:**

* Blower Door kit
* IR imager
* Manometers and hoses
* Combustion Analyzer (measures CO, oxygen and temperature)
* Hand held CO detector (if not a feature on combustion analyzer)
* Gas leak detector
* Smoke generating device
* Probe thermometers
* Pressure pan
* Exhaust fan flow meter
* “Watts Up” meter
* Inspection mirrors.
* Bore scope
* Digital camera (most will bring their own)
* Pads of paper and pencils

**Assorted Tools and Material:**

* + Telescoping ladder – lightweight and convenient; easy to maneuver in tight quarters.
  + Cordless drill with drill bits and assorted drivers
  + Long probe gas grill lighter
  + Non contact voltage detector
  + Phillips head and slotted screwdrivers.
  + Cutting pliers.
  + Regular gripping pliers
  + Hammer
  + Awl punch
  + Adjustable wrench.
  + Assorted fasteners
  + Box Cutter.
  + 25’ tape measure.
  + Flashlight
  + Utility light (electric)
  + Plastic crochet hook (for fishing insulation samples through small openings).
  + Clear sticky duct masking (to cover registers)
  + Wide painters masking tape
  + Duct tape
  + Electrical tape
  + Extension cord in 25 or 50 foot lengths
  + Power strip
  + Three prong electrical outlet adapter

PPE:

* Tyvec suits
* Roll plastic
* Hand sanitizer
* Protective eye glasses
* Industrial first aid kit
* Line voltage detector